**DWR966 GPL code Test Report**

F/W: DWR-966\_GPL\_v103CP.tar.gz

MD5 checksum: 984201bed6e1ff147c438f1b3faaac4a

Version: v1.0.3CP

Test environment

|  |  |  |
| --- | --- | --- |
| Test OS | RD request OS | Test Result |
| Ubuntu 12.04.5 LTS (i386) | Ubuntu 12.04.5 LTS (i386) | Pass |

Compile GPL source code

|  |  |
| --- | --- |
| Test Item | Test Result |
| Check the compile steps of readme file. | Pass |
| Add scrip to record compile command(**console output**) | Pass |
| F/W can be compiled successfully. | Pass |
| The image can be loaded into device successfully. | n/a |
| The Web UI can be accessed successfully. | n/a |
| Check the HW & FW version(capture image) | n/a |
| Check the firmware version of hidden page | n/a |
| Restore formal released Firmware to DUT | n/a |

Some items above are n/a, because the image should be encrypted by a private key then can be loaded to device. However the key should not be published.

Note: compile command: choice one of below commands.

1. $ make
2. $ make V=99 (for detail compile information)
3. $ make V=99 > compile.log (if you want to record the compile log)